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Table S1 - Available metadata for biosolid samples collected from 7 WWTPs in Ireland. AD = Anaerobic Digestion; TD = Thermal Drying; THP = Thermal Hydrolysis Processing; P = Pasteurization; LS = Lime Stabilisation.	Comment by Scilight: We changed it to Table S1, please confirm.
	WWTP Site Reference #
	Population Equivalent (PE) Band
	Output Flow Band (m3/day)
	Types of Biosolids Treatment

	WWTP 1
	> 100,000
	> 30,000
	Advanced AD

	WWTP 2
	> 100,000
	> 30,000
	AD, TD

	WWTP 3
	> 100,000
	> 30,000
	AD, TD

	WWTP 4
	>100,000
	>30,000
	THP, AD

	WWTP 5
	2,000 - 50,000
	1,000 - 10,000
	AD, P

	WWTP 6
	2,000 - 50,000
	1,000 - 10,000
	AD, TD

	WWTP 7
	50,000-100,000
	10,000 - 30,000
	LS



